LW Tool Chain
Prev |  | Next

# Chapter 2. Output Formats

The LW tool chain supports multiple output formats. Each format has its advantages and disadvantages. Each format is described below.

# 2.1. Raw Binaries

A raw binary is simply a string of bytes. There are no headers or other niceties. Both LWLINK and LWASM support generating raw binaries. ORG directives in the source code only serve to set the addresses that will be used for symbols but otherwise have no direct impact on the resulting binary.

Prev | Home | Next
Introduction |  | DECB Binaries